{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["表-08 分部分项工程和单价措施项目清单与计价表(含措施标题)"],"read":"whole","date_system":"1900"}

{"sheet":"表-08 分部分项工程和单价措施项目清单与计价表(含措施标题)","index":0,"n_rows":22,"n_cols":10,"rows_kept":22,"merged":[[0,0,0,9],[1,0,1,2],[1,3,1,6],[1,7,1,9],[2,0,4,0],[2,1,4,1],[2,2,4,3],[2,4,4,4],[2,5,4,5],[2,6,2,9],[3,6,4,7],[3,8,4,8],[5,2,5,3],[5,6,5,7],[6,2,6,3],[6,6,6,7],[7,2,7,3],[7,6,7,7],[8,2,8,3],[8,6,8,7],[9,2,9,3],[9,6,9,7],[10,2,10,3],[10,6,10,7],[11,2,11,3],[11,6,11,7],[12,2,12,3],[12,6,12,7],[13,2,13,3],[13,6,13,7],[14,2,14,3],[14,6,14,7],[15,2,15,3],[15,6,15,7],[16,2,16,3],[16,6,16,7],[17,2,17,3],[17,6,17,7],[18,2,18,3],[18,6,18,7],[19,2,19,3],[19,6,19,7],[20,2,20,3],[20,6,20,7],[21,0,21,7],[22,0,22,9],[23,0,23,2],[23,3,23,6],[23,7,23,9]]}
["工程量清单"]
["工程名称：质检楼403室装修改造"]
["序号","项目名称","内容",null,"计量单位","工程量","金额（元）"]
[{"$nulls":6},"综合单价",null,"综合合价","其中"]
[{"$nulls":9},"暂估价"]
["1","玻璃隔断","1.边框材料种类、规格:“83款”成品单玻铝合金隔断\n2.玻璃品种、规格、颜色:12mm钢化玻璃",null,"m2",80]
[2,"吊轨推拉门","1.门框或扇外围尺寸分别为:1.2*2.1m、 3.0*2.1m\n2.框、扇材质:吊轨门\n3.玻璃品种、厚度:12mm钢化玻璃\n4.形式：双开趟门\n5.安装位置：办公区与制样区隔断",null,"扇",2]
[3,"地弹门","1.门框或扇外围尺寸分别为:1.4*2.1m\n2.框、扇材质:地弹门\n3.玻璃品种、厚度:12mm钢化玻璃\n4.形式：平推双开门\n5.安装位置：制样干区与制样湿区隔断",null,"扇",1]
[4,"环氧树脂实验台","1.全钢结构实验台框架\n2、黑色环氧树脂实验台面\n3、台面边缘加挡水条",null,"m2",5]
[5,"实验室水槽","1.材质:塑料\n2.规格、类型:普通\n3.安装要求：满足实验室使用4.边缘加挡水条",null,"个",2]
[6,"给水管","1.安装部位:室内\n2.介质:废水\n3.材质、规格:De50\n4.连接形式:热熔连接",null,"m",15]
[7,"排水管","1.安装部位:实验室水槽排水管\n2.介质:废水\n3.材质、规格:De50\n4.连接形式:热熔连接",null,"m",15]
[8,"插座","1.名称:16A插座安装\n2.安装方式:安装在实验台上\n3.安装要求：重新敷设管线",null,"个",10]
[9,"通风橱拆除","1.构件名称:通风橱\n2.拆除要求：拆除后需做好原有通风管道处理，并搬至指定位置(拆8个，装4个）",null,"台",12]
[10,"干湿区分界.实验台台面电柱拆除","1、原有试验台面插座拆除\n2、隔断安装完毕后，按现场需求重新安装插座\n3、安装方式：明装\n4、材质：PVC",null,"项",1]
[11,"天花恢复","1.天花类型:矿棉多孔天花\n2.龙骨类型:轻钢龙骨",null,"m2",15]
[12,"管线整理（包含空调移位）","1.天花内管线复位\n2、整理天花内无套管管线\n3、空调移位等\n4、空调移位后天花修复",null,"项",1]
[13,"垃圾清理","1.清理施工中所有垃圾及拆除中产生的垃圾",null,"项",1]
[14,"试验台加装挡水条","1.原有现场试验台台面边缘加装挡水条",null,"项",1]
[15,"施工措施费用","1.脚手架\n2、安全文明施工措施",null,"项",1]
[null,"分部分项合计"]
["本页小计"]